You are here: Introduction > Configuration Methods and Intel AMT Versions

# Configuration Methods and Intel AMT Versions

There are many different versions of Intel AMT. This table gives the configuration methods available for the different Intel AMT versions.

# | Configuration Method | Intel AMT Versions
--- | --- | ---
1 | Host-based Configuration | 6.2 and higher
2 | SMB/Manual Configuration | 4.0 and higher
3 | One-Touch Configuration using PSK | 2.1 and higher
4 | Remote Configuration using PKI | 2.2, 2.6, 3.0 and higher
Configuration methods #3 and #4 are not supported by the Configuration Utility. These configuration methods use the Remote configuration Service (RCS) component of Intel SCS. For more information about Intel SCS, refer to the Intel(R)_SCS_User_Guide.pdf.